{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":4,"rows_kept":5,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["采购内容"]
["序号","材料名称","规格型号","备注"]
[1,"轻质耐酸浇注料","常温耐压强度16(MPa），  体积密度1400kg/m³"]
[2,"耐酸防腐涂料","OM：耐酸性大于等于96%，粘结强度：1.7MPA,质量等级一级，刷2遍"]
[3,"玻璃丝布","拉伸断裂强力（横纵）13.5N，150mm*200mm"]