{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":4,"rows_kept":6,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["采购内容"]
["序号","材料名称","规格型号","备注"]
[1,"1路灯光面板","CS-HAL-SW21C-01NWG","1.工作电压:240V~50Hz \n2.设备功耗:待机功耗0.5W\n3.负载功率:白炽灯1000W、节能灯/日光灯200W\n4.无线通信协议:ZigBee 3.0\n5.无线发射功率:20dbm\n6.无线接收灵敏度:-104dbm\n7.产品尺寸:86*86*36mm\n8.安装方式:86底盒(最小深度55mm)"]
[2,"2路灯光面板","CS-HAL-SW21C-02NWG","1.工作电压:240V~50Hz \n2.设备功耗:待机功耗0.5W\n3.负载功率:白炽灯1000W、节能灯/日光灯200W\n4.无线通信协议:ZigBee 3.0\n5.无线发射功率:20dbm\n6.无线接收灵敏度:-104dbm\n7.产品尺寸:86*86*36mm\n8.安装方式:86底盒(最小深度55mm)"]
[3,"3路灯光面板","CS-HAL-SW21C-02NWG","1.工作电压:240V~50Hz \n2.设备功耗:待机功耗0.5W\n3.负载功率:白炽灯1000W、节能灯/日光灯200W\n4.无线通信协议:ZigBee 3.0\n5.无线发射功率:20dbm\n6.无线接收灵敏度:-104dbm\n7.产品尺寸:86*86*36mm\n8.安装方式:86底盒(最小深度55mm)"]
[4,"2路场景面板","CS-HAL-SW22C-04NWG","1.工作电压:240V~50Hz \n2.设备功耗:待机功耗0.5W\n3.无线通信协议:ZigBee3.0\n4.无线发射功率:20dbm.\n5.无线接收灵敏度:-104dbm\n6.产品尺寸:86*86*36mm\n7.安装方式:86底盒(最小深度55mm）"]