{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":4,"rows_kept":4,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["采购内容"]
["序号","材料名称","规格型号","备注"]
[1,"移动泵车","CH2000-10型油电两用移动泵车\n1.潍柴动力或同等质量品牌120KW\n2.4台流量：500m3/h、扬程：10m便携式潜水泵\n3.电启动，仪表显示控制系统\n4.22KW变频启动柜\n5.移动拖车：四轮拖车底盘，四支撑脚\n6.2mm镀锌钢板+户外型喷塑烤漆防风雨箱体\n7.一体式公共底座\n8.底座油箱\n9.80Ah免维护蓄电池及连接线\n10.工业消音装置\n11.浮箱\n12.DN200消防水带1根（20/根）+快速接头\n13.机组，发动机，水泵等工具包"]
[2]