{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":4,"rows_kept":3,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["采购内容"]
["序号","材料名称","规格型号","备注"]
[1,"移动泵车","1，潜水永磁泵3台:8寸，流量:612m3/h、扬程:8m，电机功率22KW(每台泵含电缆线30米)\n2，柴油发电机组1台:150KW.电压 400/230V，频率50HZ\n3,塑料浮船3台套。\n4,移动拖车1套: 车中置4轮(8胎)汽车轮胎,四腿支撑脚,牵引架,强度按 40km/h校核，整车(长*宽*高>4000mm*2000*2200)。\n5，防风雨箱体1套:全车封闭防风雨箱采用2mm户外型喷塑烤漆，6开门液压支杆。\n6，出水管:DN200水带3盘(每盘出水管50米)\n7，燃油油箱1个(底座油箱)，4腿支撑1套，安全绳，救生衣各一套。蓄电池1套:100Ah免维护蓄电池及连接线(2块电瓶)8.9.变频控制柜1台(一控三)，手机远程遥控水泵启动和停止。10，救生绳，水裤，救生衣和救生圈各一套11，三方检验报告，合格证各1份。"]