{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["采购内容"]
["序号","材料名称","规格型号","备注"]
[1,"平板铸铁闸门","PZ1*1（单扇闸门重：0.6t）"]
[2,"直柄手推式螺杆启闭机","QLC-10A（单台启闭机重：0.245t）"]
[3,"平板铸铁闸门","PZ2*1（单扇闸门重：1.2t）"]
[4,"直柄手推式螺杆启闭机","QLC-30A（单台启闭机重：0.742t）"]
[5,"风光结合智能一体化闸门","1*1（含摄像头、智能监控系统、风光互补供电系统等配套设备）"]
[6]
[7]
[8]
[9]
[10]