{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"merged":[[0,0,0,3],[2,3,11,3]],"flags":["formulas_cached_only"]}
["采购内容"]
["序号","材料名称","规格型号","备注"]
[1,"铸铁闸门","1.5*1","以上启闭机螺杆材质均为Q235B,QL-3t启闭机螺杆直径46,QL-5t启闭机螺杆直径51，高度1米闸门配的启闭机螺杆长2.6米，高度1.5米闸门配的启闭机螺杆长3.1米，高度2米配的启闭机螺杆长3.7米"]
[2,"铸铁闸门","1*1"]
[3,"铸铁闸门","1.5*1.5"]
[4,"铸铁闸门","2*1"]
[5,"铸铁闸门","2*1.5"]
[6,"铸铁闸门","2*2"]
[7,"铸铁闸门","2.5*2"]
[8,"铸铁闸门","1*1.5"]
[9,"启闭机","QL-3t手电一体"]
[10,"启闭机","QL-5t手电一体"]